# OctopusNet

Layer 2 Quality of Service |  | See note below
Telnet |  | Enable it at your own risk
NODMS |  | Disable DMS announcement.
NODVBT |  | Disable DVBT announcement.
No DVB switch |  | Disable DVB switch emulation on S8.

### Layer 2 Quality of Service

This is defined in the IEEE 802.1Q VLAN standard, and provides QoS in a local network.
For it to work all components in the LAN must either be transparent to it or need to support it.
- hubs: always transparent.
- dumb switches: usually transparent, better ones use it to prioritise the traffic.
- smart switches: depends on setting.
- PCs and the like: newer systems support it by default, for older systems check the LAN adapter settings.
- WLAN access points: depends on firmware and model. OpenWRT based devices usually work.
Dies ist im IEEE 802.1Q VLAN Standard definiert und erlaubt QoS im lokalem Netz.
Damit es funktioniert müssen alle Netzwerkkompenenten im LAN entweder transparent sein oder es unterstützen.
- Hubs: sind immer transparent
- Dumb Switches: normalerweise transparent, bessere prioritisieren damit den Datenverkehr
- Smart Switches: hängt von den Einstellungen ab
- PCs und dergleichen: neue Systeme unterstützten es defaultmässig, für ältere in den Einstellungen der Netzwerkarte nachschauen
- WLAN Accesspoints: hängt von Modell und deren Firmware ab. OpenWRT basierte Geräte unterstützen es normalerweise